Formulari Nr. 3

[image: ]FTESË PËR OFERTË

Emri dhe adresa e autoritetit kontraktor
Emri ______Bashkia  Memaliaj___
Adresa :Memaliaj
Tel/Fax____0686303730__
E-mail______bashkiamemaliaj@gmail.com
Faqja e Internetit____x

Autoriteti kontraktor do të zhvillojë procedurën e prokurimit me vlerë të vogël me fond limit 730 000 (SHTATEQIND E TRIDHJETE MIJE ) LEKE
Objekti: Blerje paisje topografike    per nevoja te   Bashkise  Memaliaj   .
Data e zhvillimit do të jetë  11.05.2016 ,ora ___10.00_____në adresën www.app.gov.al 

Jeni të lutur të paraqisni ofertën tuaj për këtë objekt prokurimi me këto të dhëna (specifikimet teknike të mallit/shërbimit/punës):
Operatori ekonomik i renditur i pari, i cili shpallet fitues, duhet të dorëzojë pranë autoritetit kontraktor (në rastet kur kërkohet), dokumentet si më poshtë:
1.Licence konform legjislacionit ne fuqi( Ekstrakt nga QKR)
2. Vertetim per shlyerje te energjise elektrike nga OSHEE. 
3.Vertetim per shlyerjesh detyrime tatimore  ne njesine ku ushtron aktivitetin.
Cdo dokument ka  vlere   brenda nje periudhe  3-mujore nga data e paraqitjes.

Operatori ekonomik i renditur i pari, duhet të paraqitet pranë autoritetit kontraktor  deri date  13.05.2016  ora  10.00   .
      (data dhe ora e përcaktuar nga autoriteti kontraktor)

Afati i lëvrimit të mallit/realizimit të shërbimit/punës do të jetë data 16.05.2016-21.05.2016
 (te plotësohet nga autoriteti kontraktor).

	PREVENTIV
BASHKIA MEMALIAJ
Blerje Paisje Topografike
Fondi limit (pa TVSH)= 730,000 lek
	
Nr
	
Nr.An
	
EMERTIMI I PUNIMEVE
	
NJESI
	
SASI
	
ÇMIMI
	
VLEFTA

	1
	
	  Reflectorless Construction Tachymeter
 
	cope
	1
	
	

	2
	
	Nivele vetehorizontuese  e kompletuar
	cope
	1
	
	

	3
	
	GPS dore me saktësi deri 1 – 3 m
	cope
	1
	
	

	4
	
	Matës distancash dore me rreze  
	cope
	1
	
	

	5
	
	   Aparat fotografik 
   EOS Rebel T6 EF-S 18-55mm f/3.5-5.6 IS II Kit

EOS Rebel T6 EF-S 18-55mm f/3.5-5.6 IS II Kit


 
	cope
	1
	
	

	6
	
	Metra shirit deri 50 m  
	copee
	1
	
	

	7
	
	Metra  30 m
	cope
	6
	
	

	
	Shuma Totale pa TVSH
	


Tv sh 20 %	   
To[image: ]tali	
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Fondi limit pa TVSH eshte  730 000 leke.
Në ofertën e tij, ofertuesit duhet të paraqesë të dhënat e plota të personit të kontaktit.
SPECIFIKIME TEKNIKE

1.Reflectorless Construction Tachymeter 1 COP

Reflectorless Construction Tachymeter
Matje ne tre dimensional. X, Y, Z
Matje direkte me Lazer 200 metra ose me shume 
Menu te thjeshte per te kursyer kohe
Pike lazer per te gjetur lehtesisht targetin
Qenderzim me lazer per stacionim me te shpejte
Matje me prizem 600 metra ose me shume
Matje e vijes se munguar: Kalkulim Distance te pjerret, Distance horizontale, Lartesie Vertikale dhe diference mes 2 pikave.
Offset: Kalkulim distance dhe kendi ne rraport me piken e matur 
REM: Matje ne menyre indirekte te lartesise se objekteve kur metoda direkte nuk mund te kryhet
Resection: Kryen stacionim te instrumentit duke lexuar 2-10 pika me koordinata te njohura (Free Station)
Area: Kalkulim siperfaqe me minimumi 3 pika.
Transferim i te dhenave ne kompjuter me ane te fishave dhe softwari te lejoje ruatjen ne formate te ndryshme si .dxf ne menyre qe te mund te importohet direkt ne AutoCAD
Me shume se 26 butona
Memorie 50,000 pika
SPECIFIKIME 
	Telescope
	

	Image
	Erect

	Objecitve aperture (EDM)
	45 mm

	Magnification
	30 x

	Field of view
	1° 30' 

	Resolving power
	4''

	Shortest focussing distance
	1,5 m

	Distance measurement
	

	Refl ectorless
	1 bis 200 m

	Flat prism FP 50
	1 bis 600 m

	Reflective tape target RS
	1 bis 600 m

	Single standard prism 62 mm
	1 bis 600 m (Offset = 0)

	A[image: ]ccuracy
	3 mm + 2 ppm

	Measuring time
	

	(fine / rapid / tracking)
	1,5 s / 0,9 s / 0,3 s

	Minimum reading
	1 mm

	Units
	ft / m

	Angle measurement
	

	Minimum reading resolution steps
	1'' / 5'' / 10''

	Accuracy
	5''

	Angle units
	100 % / 360° / 400gon

	Compensator
	

	Type
	Electronical

	Range
	± 3°

	Laser Pointer
	

	Laser class
	3R

	Laser plummet
	

	Accuracy
	± 1 mm / 1,5 m

	Laser class
	2

	Display
	

	Dual LCD
	4 lines, 24 characters

	Power supply
	

	Rechargeable battery
	7,2 V DC NiMH

	Operating time
	5 h

	Charger
	100/240 V

	Vial sensivity
	

	Plate level vial
	30'' / 2 mm

	Circular vial
	8' / 2 mm

	General
	

	Internal memory capacity 
	50.000 Points

	Weight (instrument)
	6,0 kg

	Operating temperature
	-20°C bis +50°C

	Dust / water protection
	IP 54 

	I/O-Port
	RS-232


2. GPS dore me saktësi deri 1 – 3 m.  1 cope
GPS me ekran me prekje, GPS& GLONNAS, 3-axis Compass, Barometric Altimeter
· 2.6-inch color capacitive touchscreen
· 3-axis tilt-compensated compass and barometric altimeter
· GPS and GLONASS satellites for faster positioning
· 4 GB memory to hold more maps,
· Koordinata metrike ne sistemin Shqiptar. 
· Harte e Shqiperise me IZOIPSE cdo 10m 

3. Matës distancash dore me rreze deri 120m.  1 cope
Features
· Minimum / maximum
· Permanent[image: ] measurement
· Plus / minus
· Area / volume
· Room function summary
· Height measurement (Pythagoras)
· Measurement despite obstructions
· Stake-out function
· 360° tilt sensor
· mm, ft, inch
· Multi-functional endpiece
Range and accuracy test according to ISO 16331-1
Technical data
	Distance
	0,05 – 120 m

	Accuracy
	± 1,0 mm

	Dust / water protection
	IP 65 

	Weight
	155 g

	Laser class
	2

	
	



4-Aparat fotografik  1 cope.
· EOS Rebel T6 EF-S 18-55mm f/3.5-5.6 IS II Kit
· https://www.usa.canon.com/internet/portal/us/home/products/details/cameras/dslr/eos-rebel-t6-ef-s-18-55mm-is-ii-kit

5- Meter Shirit 50m   cope 1
6. Meter Shirit Xhepi  30 M cope 6
7. Nivele vetehorizontuese  e kompletuar ,stativ,late etj . cope 1
Technical data
	Mean error for 1 km double leveling
	1,0 mm

	Telescope magnification
	32 x

	Objective diameter
	38mm

	Shortest focussing distance
	0,3m

	Working range of compensator 
	±15'

	Levelling accuracy
	±0,5

	Circular bubble
	8'/2mm

	Horizontal circle
	400 gon/360°

	Dust / water protection
	IP 54

	Weight
	1,5 kg



Shenim: Operatori Ekonomik ofertues duhet te jete i certifikuar me standartin ISO 9001:2008 p[image: ]er Shitjen dhe Trajnimin e paisjeve Topografike. Si dhe te paraqese çertifikata trajnimi per Instrumentat Topografik.
Garancia e materialeve  jo me pak se  2 vjet.
  
PER SEKTORIN E ZHVILLIMIT URBAN DHE KADASTRES
/ing.Violeta Kanushi/        /Andrea  Çoka/


TITULLARI I AUTORITETIT KONTRAKTOR /OSE PERSONI I AUTORIZUAR PREJ TIJ

Durim Rroshi
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